PwrButton long press
dwPwrbtnLongPressFunc=8
++++++HandlePopPwrDlg++++++
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++ShowPic++++++
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDeco++++++GenDispInfo++++++
------GenDispInfo------
derIsSignalLocked------[0] 
------ShowPic------
mute wav out
Wavproxy wavout dev=1, wavein dev=1
Wavproxy wavout dev=2, wavein dev=2
pwr:get Cmmb quit!
Touch: do real power down
DeinitTscAdc=0x1
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
===>Unload driver Drivers\CSR\BcspDrv with index 0
[PWM_Open][447]++
[PWM_Open][448]--
[PWM_IOControl][586]++
PWM_IOControl: Recevied IOCTL 40fa4 =IOCTL_PWM_DISABLE_PORT
 PwmPort = (0), PwmDutyCycle = (50)
[PWM_IOControl][1076]--
[PWM_Close][463]++
[PWM_Close][464]--
[BTP][BTChipPowerOff] Close BT_32K_CLK from PWM0
[BTP][BTChipPowerOff] Close BT_CLK
[BTP][BTChipPowerOff] BT power enable through GPIO2[24]
IOCTL_POWER_SET:power down
CHW::PowerMgmtCallback(SUSPEND)CRootHub::SuspendNotificationInPowerHandler(exit)
CHW::PowerMgmtCallback(SUSPEND) exit
UsbSocHnpPhyClk: 0.
[COM_IOControl]: power status: D3.
[COM_IOControl]: WAITING TO ENTER POWER STATE.
[COM_IOControl_Sleep]: waiting for SOCNAV_STOP_Engine()...
platformGpsRfPowerOff: AtlasVI OEMGpsRFPowerOFF., 
PP has lost power  
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
++++++HwDecoderIsSignalLocked++++++ 
------HwDecoderIsSignalLocked------[0] 
[COM_IOControl_Sleep]: SOCNAV_STOP_Engine() successfully.
RF has lost power
PP has lost power  
RF has lost power
PP has lost power  
[COM_IOControl_Sleep]: GPS sleeps successfully.
[COM_IOControl]: LEAVING POWER STATE.
IOCTL_POWER_SET, D3, D4
IOCTL_POWER_SET, D3, D4
USP is disabled, dwUspIndex=3
Set Backlight Power state: 3
[PWM_Open][447]++
[PWM_Open][448]--
[PWM_IOControl][586]++
PWM_IOControl: Recevied IOCTL 40fa0 =IOCTL_PWM_ENABLE_PORT
IOCTL: PwmFlag = 1, PwmPort = 2, PwmSourceClk = 3, PwmOutputFreq = 400, PwmDutyCycle = 100
 dwHigh=81, dwLow=0 ,dwPrecision=99
[PWM_IOControl][1076]--
[PWM_Close][463]++
[PWM_Close][464]--
kernel PVRSRV_IOCTL_POWER_SET setting state 3
[DSK_IOControl][1320]: Nand Controller Power Down 
[WaitForSessionDone][801]: Power function call, keep the lock
Powering Off system:
  Calling GWES power proc.
Enter CspCmnGPE::PowerHandler bOff=1
Leave CspCmnGPE::PowerHandler
  Calling device manager power proc.
++++++NUM_PowerDown++++++
------NUM_PowerDown------
OTG_PowerDown
+PFM_PowerDown(0xd037ecf4 )
DeinitTscAdc=0x0
[PWM_PowerDown][543]++
[PWM_PowerDown][544]--
UTLDRV::UTL_PowerDown()!
  Calling OEMPowerOff...
OEMPowerOff
WARNING: Still has DMA channel working: DMA1_CH_VALID 0x100!
HalLockCode+++0x88f21000+++1++HalLockCode-